# Car Door Hinge Lubrication

This playbook outlines the steps required to lubricate car door hinges effectively. The goal is to eliminate squeaking noises and ensure the door operates smoothly.

### Step 1: Gather Supplies

Collect the necessary materials for the task: a can of WD-40 or suitable lubricant spray, a rag or paper towels, and protective gloves.

### Step 2: Prep Area

Open the car door and use the rag or paper towels to clean around the hinge area, removing any dirt or debris that might be present.

### Step 3: Apply Lubricant

Shake the lubricant can well before use. Then, spray a small amount directly onto the car door hinges. Be careful not to overspray onto the car's body or interior.

### Step 4: Work Hinges

After applying the lubricant, slowly open and close the door several times to work the lubricant into the hinge mechanism.

### Step 5: Wipe Excess

Use a clean rag or paper towel to wipe off any excess lubricant from the hinge area to prevent dirt accumulation.

### Step 6: Test Door

Open and close the door several times to ensure that the squeaking has stopped and the door is swinging smoothly. Repeat lubrication if necessary.

## General Notes

### Safety

Wear protective gloves to keep your hands clean and avoid contact with the lubricant, which may be harmful to skin.

### Environmental Care

Use the lubricant in a well-ventilated area and dispose of any used rags or paper towels properly to minimize environmental impact.